Skip to main content

# Device List

## Before You Start​

1. On each device, enable `More → Remote Access` in the XXTouch app.
2. Make sure the devices and the control center are on the same LAN, and that the control center machine allows the default ports through the firewall.
3. If the control center runs behind Docker or a reverse proxy, confirm that devices can still reach it correctly.

## Discovering and Importing Devices​

- Broadcast scan: `Scan and Refresh` is the quickest way to discover devices on the current LAN.
- Import device list: the import panel supports subnet-based scans and single IP imports.
- Bulk paste from clipboard: if you already have a list of IPs, you can paste them directly into the import panel.
- Retry failed devices: failed imports can be retried from the same panel.
- Switch subnets: you can switch to another subnet and continue scanning without leaving the main app.
- Import groups: imported devices can be grouped by import batch to keep them easier to manage later.

## Selecting Devices​

- Click a device row or checkbox to select it.
- Select one device, then hold `Shift` and click another row to select the full range between them.
- Selecting a group changes the current operation scope, but it does not automatically check every device row. If you want to run an action on all devices, you still need to select them in the device list.

## Columns and Logs​

- Use the header settings menu to choose which columns are visible.
- `Log #1` to `Log #6` can each have a custom alias, so you can rename them to match your workflow.
- You can open log history from the device context menu or from remote control panels.

## Common Context Menu Actions​

- Add selected devices to a group
- Batch rename devices or delete device records
- Browse device files
- Open single-device remote control
- Capture a screenshot and open it in the Color Picker
- Add currently selected devices to the batch remote control panel when it is already open