Skip to main content

# Remote Control and Batch Remote Control

XXTLanControl provides both single-device remote control and batch remote control. Both are designed around live screen streaming and real-time control.

## Single-Device Remote Control​

From the device list, right-click a device and choose `Remote Control`.

Common actions include:

- live screen viewing
- mouse or touch input
- keyboard input and common key forwarding
- screenshots
- clipboard read and write
- device log access

If you only need a screenshot for color picking, you do not have to enter the full remote control panel. You can use `Capture Screenshot and Open in Color Picker` directly from the context menu.

## Batch Remote Control​

1. Select multiple devices on the main screen.
2. Open `More Actions → Batch Remote Control`.
3. Use the batch remote control panel to view and operate those devices together.

This panel is useful for:

- watching many device screens at once
- broadcasting touch or key input to selected sync targets
- sending text clipboard content to many devices
- sending image clipboard content to many devices
- capturing screenshots and opening them in the picker workbench
- opening logs, device files, or single-device remote control from each device card

If the batch remote panel is already open, you can go back to the device list and add more selected devices into it.

## Screenshot Saving​

- Screenshots can be saved back into the control center so they are easy to keep and reuse.
- If you want to save images directly to a folder on your computer, enable the related local-save permission in `Settings` and open the console on the same machine.

## Related Entries​

- Browse Device Files: useful for pulling scripts and resources from a device
- View Log History: useful for debugging device-side script output
- Picker Workbench: useful when you want to continue working with screenshots after capture